{
    "board_id": 1150,
    "magic": "APJFWv1",
    "description": "Firmware for a STM32F405xx board",
    "image": "[encoded data, 787484 characters]",
    "extf_image": "eNoDAAAAAAE=",
    "summary": "MicoAir405v2",
    "version": "0.1",
    "image_size": 855372,
    "extf_image_size": 0,
    "flash_total": 999424,
    "image_maxsize": 999424,
    "flash_free": 144052,
    "extflash_total": 0,
    "extflash_free": 0,
    "git_identity": "960ca66d",
    "board_revision": 0,
    "USBID": "0x1209/0x5741"
}